This is Release Candidate 1 (RC1) of the visor frame for the face shield PPE.

The design has been optimised to stack with a 0.25 gap.

Makerbot print settings are set up with a 0.25 layer height, padded base, 3 shells, 10% infill. Note that the layer height must correspond with the gap if you wish to change it.

Please check the attribution text for crediting/attributing.